{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Schmutz F"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schmutz F","index":0,"n_rows":36,"n_cols":22,"rows_kept":36,"cut":false,"hidden":false,"merged":[[1,10,1,11],[2,10,2,21],[3,3,3,21],[1,12,1,20],[2,8,2,9],[1,3,1,4],[1,8,1,9],[2,3,2,4],[1,0,1,2],[2,0,2,2],[3,0,3,2],[1,5,1,7],[2,5,2,7],[6,0,7,2],[4,3,5,11],[4,12,5,20],[4,21,5,21],[35,3,35,9],[35,12,35,18],[4,0,5,2]]}
[]
["GÉNIE CIVIL   BIENNE",null,null,"N° DPC",null,"                    ",null,null,"Parc. Nr.",null,"                                                                                                                  ",null,"WAS = Eaux  usées  /  Eaux  mélangées",null,null,null,null,null,null,null,null,1]
["Évacuation  des  eaux  des  biens-fonds",null,null,"N° DPE",null,"               ",null,null,"Rue"]
[" PROPRIÉTAIRE  FONCIER"]
["Récapitulation unités de raccordement                                 bâtiment / eaux usées ",null,null,"ÉTAT RÉEL",null,null,null,null,null,null,null,null,"NOUVEL  ÉTAT",null,null,null,null,null,null,null,null,"Contrôle"]
[]
["Niveau",null,null,"S.-S.","RC",1,2,3,4,null,"Nbre.","Total","S.-S.","RC",1,2,3,4,null,"Nbre.","Total"]
[null,null,null,null,null,null,null,null,null,null,"org. évac.","UR",null,null,null,null,null,null,null,"org. évac.","UR"]
["Lm","Lave-mains, lavabo  jusqu'à  3  robinets",0.5,null,null,null,null,null,null,null,{"$f":"SUM(D9:J9)","v":0},{"$f":"K9*C9","v":0},null,null,null,null,null,null,null,{"$f":"SUM(M9:S9)","v":0},{"$f":"T9*C9","v":0}]
[null,"                                        "]
[null,"                                               "]
["B","Baignoire",1,null,null,null,null,null,null,null,{"$f":"SUM(D12:J12)","v":0},{"$f":"K12*C12","v":0},null,null,null,null,null,null,null,{"$f":"SUM(M12:S12)","v":0},{"$f":"T12*C12","v":0}]
["D","Receveur  de  douche",null,null,null,null,null,null,null,null,{"$f":"SUM(D13:J13)","v":0},{"$f":"K13*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T13*C12","v":0}]
["U","Urinoir, pissoir                ",null,null,null,null,null,null,null,null,0,{"$f":"K14*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T14*C12","v":0}]
[null,"Lave-mains, 4 à 10  robinets",null,null,null,null,null,null,null,null,0,{"$f":"K15*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T15*C12","v":0}]
[" ","Plonge, évier  de  cuisine",null,null,null,null,null,null,null,null,0,{"$f":"K16*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T16*C12","v":0}]
["EV","Plonge  double, lavabo  double",null,null,null,null,null,null,null,null,0,{"$f":"K17*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T17*C12","v":0}]
[null,"Bassin  de  buanderie, buanderie",null,null,null,null,null,null,null,null,0,{"$f":"K18*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T18*C12","v":0}]
[" ","Lave-vaisselle  de  ménage"," ",null,null,null,null,null,null,null,0,0,null,null,null,null,null,null,null,0,0]
["LI","Lave-linge  de  ménage  jusqu'à  6 kg.",null,null,null,null,null,null,null,null,0,{"$f":"K20*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T20*C12","v":0}]
["GS","Grille-siphon  DN  57",null,null,null,null,null,null,null,null,0,{"$f":"K21*C12","v":0},null,null,null,null,null,null,null,0,{"$f":"T21*C12","v":0}]
[null,"                                         "]
[null,"                                            "]
[" ","Lave-vaisselle  de  restaurant",1.5,null,null,null,null,null,null,null,{"$f":"SUM(D24:J24)","v":0},{"$f":"K24*C24","v":0},null,null,null,null,null,null,null,{"$f":"SUM(M24:S24)","v":0},{"$f":"T24*C24","v":0}]
[" ","Lave-linge  de  7  à  12 kg.",null,null,null,null,null,null,null,null,0,{"$f":"K25*C24","v":0},null,null,null,null,null,null,null,0,{"$f":"T25*C24","v":0}]
["GS","Grille-siphon  DN  69",null,null,null,null,null,null,null,null,0,{"$f":"K26*C24","v":0},null,null,null,null,null,null,null,0,{"$f":"T26*C24","v":0}]
["WC","Installations  de  WC",2.5,null,null,null,null,null,null,null,0,{"$f":"K27*C27","v":0},null,null,null,null,null,null,null,0,{"$f":"T27*C27","v":0}]
[" ","Vidoir, (eaux  fécales  et  de  nettoyage)"," ",null,null,null,null,null,null,null,0,{"$f":"K28*C27","v":0},null,null,null,null,null,null,null,0,{"$f":"T28*C27","v":0}]
[" ","Lave-linge  de  13  à  40 kg.",null,null,null,null,null,null,null,null,0,{"$f":"K29*C27","v":0},null,null,null,null,null,null,null,0,{"$f":"T29*C27","v":0}]
["GS","Grille-siphon  DN  80 - 100",null,null,null,null,null,null,null,null,0,{"$f":"K30*C27","v":0},null,null,null,null,null,null,null,0,{"$f":"T30*C27","v":0}]
[null,"Grande  baignoire, bassin  de  sauna"," ",null,null,null,null,null,null,null,0,{"$f":"K31*C27","v":0},null,null,null,null,null,null,null,0,{"$f":"T31*C27","v":0}]
[null,"                                               "]
[null,"                                             "]
[" ","                                        "," "]
[null,"                                          "]
["WAS","                                       ",null,"TOTAL  UR  ÉTAT  RÉEL",null,null,null,null,null,null,null,{"$f":"SUM(L9:L35)","v":0},"TOTAL  UR  NOUVEL  ÉTAT",null,null,null,null,null,null,null,{"$f":"SUM(U9:U35)","v":0},{"$f":"U36-L36","v":0}]